

Vortex

**QuickClear Vortex** electric suction unit is a modern, highly versatile general purpose unit designed for use across multiple applications in the commercial, hospital and community setting. Designed to meet the needs of continuous or intermittent operation, this unit combines powerful and reliable suction performance, with exceptionally quiet, maintenance free running. An ideal choice whatever the challenge.

**Features:**

* Efficient, fan cooled suction unit – reliable continuous running
* High vac, high flow – powerful suction performance
* Vibration free running at all vacuum levels – quiet unobtrusive operation
* Heavy duty, oil free double piston pump – maintenance free running
* Simple wipe clean controls – reduced contamination risk

**Technical Specification:**

|  |  |
| --- | --- |
| Vacuum Range | 0 – 680 mmHg0 – 90 kPa |
| Max. Flow Rate | 38 L/min |
| Dimensions | 440x300x310 mm |
| Weight | 12.0kg |
| Max. Noise Level | 39.4 dB |
| Warranty | 5 years |

CE marked and manufactured to EN 6061-1