

Dynamic

QuickClear Dynamic electric suction unit is the ideal choice for medical professionals seeking a high performing, reliable portable unit. Designed for use in the hospital, community or homecare setting, this unit combines a compact footprint with powerful suction performance and an exceptional 2.5 hour battery operation time.

The unit comes complete with mains charger and a 1 litre Serres canister with a disposable liner as standard (a 2 litre canister can be easily fitted if required).

**Features:**

* Two and a half hour battery run time – reliable suctioning
* High quality oil free double piston pump – powerful suction performance
* Robust, compact construction – knock proof and easy to transport
* One touch on/off button with easy to adjust vacuum control – simple to use
* Quiet performance at all vacuum levels – minimal patient disturbance
* Battery, power and charging display indicators – simple status check
* In line protection filter – prevents overflow into the unit

**Technical Specification:**

|  |  |
| --- | --- |
| Vacuum Range | 0 – 605 mmHg0 – 80 kPa |
| Max. Flow Rate | 20 L/min |
| Dimensions | 310x240x190 mm |
| Weight | 4.9kg |
| Voltage | 230V (50-60Hz)12V DC |
| Battery | Ni-Mh 3.3A (10 unit pk) |
| Run Time (Battery) | up to 2.5 hours |
| Charge Time | 4 hours |
| Max. Noise Level | 60dB |
| Warranty | 5 years |

CE marked and manufactured to EN 6061-1